From 68a31cfd621f2c8443d18433b77ae88b66b89b5b Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Fri, 30 Nov 2018 15:55:08 -0500
Subject: edit: drop cs04 changelog

move to cl-cs04.tex

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
---
 cl-os.tex | 134 +-------------------------------------------------------------
 1 file changed, 1 insertion(+), 133 deletions(-)

(limited to 'cl-os.tex')

diff --git a/cl-os.tex b/cl-os.tex
index fc12cdd..b9cc069 100644
--- a/cl-os.tex
+++ b/cl-os.tex
@@ -1,134 +1,2 @@
-540 & 11 Oct 2015 & Greg Kurz & {virtqueues: fix
-trivial typo
-
-See
-\ref{sec:Basic Facilities of a Virtio Device / Virtqueues / Used Buffer Notification Suppression}.
-} \\
-\hline
-541 & 11 Oct 2015 & Paolo Bonzini & {virtio-blk: fix typo
-in legacy framing requirements section
-
-See
-\ref{sec:Device Types / Block Device / Legacy Interface: Framing Requirements}.
-} \\
-\hline
-545 & 18 Oct 2015 & Paolo Bonzini & {virtio-blk: restore VIRTIO_BLK_F_FLUSH and VIRTIO_BLK_F_CONFIG_WCE
-
-VIRTIO_BLK_F_CONFIG_WCE is important in order to achieve good performance
-(up to 2x, though more realistically +30-40\%) in latency-bound workloads.
-However, it was removed by mistake together with VIRTIO_BLK_F_FLUSH.
-
-In addition, even removing VIRTIO_BLK_F_FLUSH was probably not a great
-idea, because it simplifies simple drivers (e.g. firmware) that are okay
-with a writethrough cache but still need data to persist after power loss.
-What really should have been removed is just the possibility that devices
-not propose VIRTIO_BLK_F_FLUSH, but even that only deserves a "SHOULD" in
-the new world of conformance statements.
-
-Restore these, with the following changes:
-
-* clarify and use conformance statements in order to define writeback
-and writethrough caching according to what is commonly done by high-end
-storage.
-
-* clarify (with conformance statements) the influence of the
-VIRTIO_BLK_F_FLUSH feature on caching and how to proceed if only one of
-VIRTIO_BLK_F_FLUSH and VIRTIO_BLK_F_CONFIG_WCE is negotiated.
-
-* strengthen the requirement for persisting writes to MUST after
-a VIRTIO_BLK_T_FLUSH request (and in other cases too involving the
-new features).
-
-The suggested behavior upon feature negotiation is okay for the Linux
-implementation of virtio1, even after the implementation is modified to
-support the two new features.
-
-This fixes VIRTIO-144.
-
-See \ref{sec:Device Types / Block Device},
-\ref{sec:Conformance / Driver Conformance / Block Driver Conformance} and
-\ref{sec:Conformance / Device Conformance / Block Device Conformance}.
-} \\
-\hline
-546 & 18 Oct 2015 & Michael S. Tsirkin & {pci: clarify configuration access capability rules
-
-The point of the configuration access capability is to enable
-access to other capabilities.  The intent never was to allow
-writes to a random place within device BARs.
-Limiting drivers simplifies devices - and devices can always
-add another capability if drivers ever want to access
-some other range.
-
-This resolves VIRTIO-145.
-
-See \ref{drivernormative:Virtio Transport Options / Virtio Over
-PCI Bus / PCI Device Layout / PCI configuration access
-capability}.
-} \\
-\hline
-547 & 18 Oct 2015 & Michael S. Tsirkin & {add advice on transition from legacy interfaces
-
-Reading legacy chapters gives a hint about what changed,
-let's help readers discover this useful shortcut.
-
-This resolves VIRTIO-146.
-
-See \ref{sec:Transition from earlier specification drafts}.
-} \\
-\hline
-554 & 16 Feb 2016 & Thomas Huth & {virtio-net: fix inconsistent legacy header size
-
-    Current text says:
-    	The legacy driver only presented num_buffers in the struct
-    	virtio_net_hdr when VIRTIO_NET_F_MRG_RXBUF was not negotiated;
-
-    Should be:
-    	"\dots was negotiated \dots" instead of "\dots was not negotiated \dots"
-
-    To be consistent with the following:
-    	without that feature the structure was 2 bytes shorter.
-
-See \ref{sec:Device Types / Network Device / Device Operation / Legacy Interface: Device Operation}.
-} \\
-\hline
-555 & 16 Feb 2016 & Michael S. Tsirkin & {virtio header: tweak
-change motivation
-
-    The changes are not just to remove Linux assumptions,
-    we have also renamed ring->queue.
-    Tweak the header description accordingly.
-
-See \ref{sec:Basic Facilities of a Virtio Device / Virtqueues / Helpers for Operating Virtqueues}.
-} \\
-\hline
-558 & 16 Feb 2016 & Michael S. Tsirkin & {rename virtio_ring.h to virtio_queue.h
-
-    Since vring* and VRING* have been replaced with virtq* and VIRTQ*
-    respectively, rename the header virtio_ring.h to virtio_queue.h.
-
-See \ref{sec:virtio-queue.h}.
-} \\
-\hline
-559 & 16 Feb 2016 & Michael S. Tsirkin & {init: sort status bits
-
-    Status bit order is inconsistent: they are neither in increasing
-    order nor in the order they are likely to be used.
-
-    The second approach seems more useful since there aren't
-    that many bits, so the numerical order does not help much.
-
-    A typical order of use would be:
-
-\begin{itemize}   
-\item    ACKNOWLEDGE
-\item    DRIVER
-\item    then either FAILED or FEATURES_OK
-\item    then either FAILED or DRIVER_OK
-\item    then DEVICE_NEEDS_RESET (if device detects an error)
-\end{itemize}
-    
-    Sort the bits accordingly.
-
-See \ref{sec:Basic Facilities of a Virtio Device / Device Status Field}.
-} \\
+REV & DATE & Author & { Description: TODO } \\
 \hline
-- 
cgit 

