From 1efcda89219390c48d249fac7d72dd2236240bc3 Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Mon, 20 Jan 2020 12:19:29 -0500
Subject: virtio-net: missing "." for feature descriptions

At end of each sentence, for consistency.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
---
 content.tex | 5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index e9d5148..f5a683d 100644
--- a/content.tex
+++ b/content.tex
@@ -2895,10 +2895,11 @@ features.
     value. Device benefits from knowing the exact header length.
 
 \item[VIRTIO_NET_F_RSS(60)] Device supports RSS (receive-side scaling)
-    with Toeplitz hash calculation and configurable hash parameters for receive steering
+    with Toeplitz hash calculation and configurable hash
+    parameters for receive steering.
 
 \item[VIRTIO_NET_F_RSC_EXT(61)] Device can process duplicated ACKs
-    and report number of coalesced segments and duplicated ACKs
+    and report number of coalesced segments and duplicated ACKs.
 
 \item[VIRTIO_NET_F_STANDBY(62)] Device may act as a standby for a primary
     device with the same MAC address.
-- 
cgit 

