From 50049af040d4af1eb69d6a2e6becf57ff52ebc7a Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Wed, 27 Nov 2019 16:26:12 -0500
Subject: virtio_pci_cap64: bar/BAR cleanups

When we mean PCI register we should say BAR.
When we mean a virtio config register we should say \field{cap.bar}.

Finally, offset_hi/length_hi are not within the cap structure.

Tweak wording slightly: "A,B,C" are fields, there's no need
to say that.

Reported-by: Christophe de Dinechin <cdupontd@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Reviewed-by: Cornelia Huck <cohuck@redhat.com>
---
 content.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index b2ebbe2..f2aea42 100644
--- a/content.tex
+++ b/content.tex
@@ -765,7 +765,7 @@ struct virtio_pci_cap64 {
 Given that the \field{cap.length} and \field{cap.offset} fields
 are only 32 bit, the additional \field{offset_hi} and \field {length_hi}
 fields provide the most significant 32 bits of a total 64 bit offset and
-length within the bar specified by \field{cap.bar}.
+length within the BAR specified by \field{cap.bar}.
 
 \drivernormative{\subsubsection}{Virtio Structure PCI Capabilities}{Virtio Transport Options / Virtio Over PCI Bus / Virtio Structure PCI Capabilities}
 
@@ -1095,9 +1095,9 @@ preference; it is only used to uniquely identify a region.
 
 \devicenormative{\paragraph}{Device-specific configuration}{Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Shared memory capability}
 
-The region defined by the combination of the \field {cap.offset},
-\field {cap.offset_hi}, and \field {cap.length}, \field
-{cap.length_hi} fields MUST be contained within the declared bar.
+The region defined by the combination of \field{cap.offset},
+\field{offset_hi}, and \field {cap.length}, \field{length_hi}
+MUST be contained within the BAR specified by \field{cap.bar}.
 
 The \field{cap.id} MUST be unique for any one device instance.
 
-- 
cgit 

