From da17c7fc4e12d3366125b12c0d7d47ddfb978cdf Mon Sep 17 00:00:00 2001
From: Paolo Bonzini <pbonzini@redhat.com>
Date: Tue, 26 Mar 2019 10:40:37 +0100
Subject: virtio_pci_common_cfg: fix field name

The field is named config_msix_vector in the rest of the document,
use the same name in the struct.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/41
Reviewed-by: Stefan Hajnoczi <stefanha@redhat.com>
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index fcce57d..5329822 100644
--- a/content.tex
+++ b/content.tex
@@ -808,7 +808,7 @@ struct virtio_pci_common_cfg {
         le32 device_feature;            /* read-only for driver */
         le32 driver_feature_select;     /* read-write */
         le32 driver_feature;            /* read-write */
-        le16 msix_config;               /* read-write */
+        le16 config_msix_vector;        /* read-write */
         le16 num_queues;                /* read-only for driver */
         u8 device_status;               /* read-write */
         u8 config_generation;           /* read-only for driver */
-- 
cgit 

