From f459b9e0ea60392f037bc740c681980563d920fc Mon Sep 17 00:00:00 2001
From: Eugenio Pérez <eperezma@redhat.com>
Date: Tue, 17 Sep 2019 09:18:03 +0200
Subject: virtio-blk: typo: Capitalization in Device Initialization item
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Eugenio Pérez <eperezma@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/51
Reviewed-by: Stefan Hajnoczi <stefanha@redhat.com>
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 5329822..b0fe90c 100644
--- a/content.tex
+++ b/content.tex
@@ -3980,7 +3980,7 @@ according to the native endian of the guest rather than
     segments for the block driver to use. \field{discard_sector_alignment}
     can be used by OS when splitting a request based on alignment.
 
-\item if the VIRTIO_BLK_F_WRITE_ZEROES feature is negotiated,
+\item If the VIRTIO_BLK_F_WRITE_ZEROES feature is negotiated,
     \field{max_write_zeroes_sectors} and \field{max_write_zeroes_seg} can
     be read to determine the maximum write zeroes sectors and maximum
     number of write zeroes segments for the block driver to use.
-- 
cgit 

