From 0b5288f06affd912f21261fc9f3a200a534fb9a5 Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Mon, 11 Mar 2019 11:48:22 -0400
Subject: signal start and end of structures consistently

Make sure all structs have the format:

struct X {
...
};

Fixes: https://issues.oasis-open.org/browse/VIRTIO-170
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Reviewed-by: Stefan Hajnoczi <stefanha@redhat.com>
Reviewed-by: Cornelia Huck <cohuck@redhat.com>
---
 virtio-gpu.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'virtio-gpu.tex')

diff --git a/virtio-gpu.tex b/virtio-gpu.tex
index 0cf2209..992d4e6 100644
--- a/virtio-gpu.tex
+++ b/virtio-gpu.tex
@@ -47,7 +47,7 @@ struct virtio_gpu_config {
         le32 events_clear;
         le32 num_scanouts;
         le32 reserved;
-}
+};
 \end{lstlisting}
 
 \subsubsection{Device configuration fields}
-- 
cgit 

