From a8b784139e10a9e2ed71243864f9b497a883de94 Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Wed, 12 Dec 2018 18:22:24 -0500
Subject: packed-ring: put normative on one line

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
---
 packed-ring.tex | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

(limited to 'packed-ring.tex')

diff --git a/packed-ring.tex b/packed-ring.tex
index 2a6c685..4395b5a 100644
--- a/packed-ring.tex
+++ b/packed-ring.tex
@@ -652,9 +652,7 @@ if (vq->device_event.flags != RING_EVENT_FLAGS_DISABLE) {
 \end{lstlisting}
 
 
-\drivernormative{\paragraph}{Sending Available Buffer Notifications}
-{Basic Facilities of a Virtio Device / Packed Virtqueues / Supplying
-Buffers to The Device / Sending Available Buffer Notifications}
+\drivernormative{\paragraph}{Sending Available Buffer Notifications} {Basic Facilities of a Virtio Device / Packed Virtqueues / Supplying Buffers to The Device / Sending Available Buffer Notifications}
 The driver MUST perform a suitable memory barrier before reading
 the Event Suppression structure occupying the Device Area. Failing
 to do so could result in mandatory available buffer notifications
-- 
cgit 

